ADMP401 Pocket Tape Orientation Change

This document refers to ADI’s Tape and Reel Packaging document, located here:

<http://www.analog.com/static/imported-files/application_notes/Tape_and_Reel_Packaging.pdf>

For all ADMP401 material produced until date code 1213, pin 1 is oriented at position C1 (illustrated below). Beginning with date code 1213 and for all material produced in the future, ADMP401 will be mounted with pin 1 oriented at position C3 (illustrated below).

