ADI PCN 13\_0217

|  |
| --- |
| ADXRS64x Die Revision R.8 QUALIFICATION RESULTS |
| Test | Specification | Sample Size | Results |
| High Temperature Operating Life (HTOL)\* | JEDEC*JESD22-A108* | **3x77** | **Pass** |
| Latch-Up | JEDEC JESD*78* | **6** | **Pass** |
| Electrostatic Discharge*Human Body Model* | ESDA/JEDEC *JDS-001-2011* | **3/voltage** | **Pass 2000V** |
| Electrostatic Discharge*Field-Induced Charged Device Model* | JEDEC *JESD22-C101* | **3/voltage** | **Pass 500V** |

\*Preconditioned per JEDEC/IPC J-STD-020