**ADP5050/52 Die Revision Qualification**

|  |  |  |  |
| --- | --- | --- | --- |
| QUALIFICATION RESULTS | | | |
| Test | Specification | Sample Size | Results |
| Latch-Up | JEDEC JESD*78* | **6** | **Pass** |
| Electrostatic Discharge  *Human Body Model* | ESDA/JEDEC *JS-001* | **3/voltage** | **Pass +/-3500V** |
| Electrostatic Discharge  *Field-Induced Charged Device Model* | JEDEC *JESD22-C101* | **3/voltage** | **Pass +/-1250V** |