|  |
| --- |
|  |

**Qualification Plan Summary**

**of ADuM7701 and ADuM7703**

|  |  |  |  |
| --- | --- | --- | --- |
| **QUALIFICATION PLAN** | | | |
| **Test** | **Specification** | **Sample Size** | **Result** |
| Electrostatic Discharge  *Field-Induced Charged*  *Device Model* | JEDEC*JS-002* | 3/voltage | Pass ±1500V |
| Electrostatic Discharge  *Human Body Model* | JEDEC *JESD22-A114* | 3/voltage | Pass ±4000V |
| Latch-Up | JEDEC *JESD78* | 1 x 15 | Pass |